From 2b9a04f904584636a5f7cd9ff2e8074320998f83 Mon Sep 17 00:00:00 2001
From: David Runge <dave@sleepmap.de>
Date: Thu, 3 Aug 2017 10:30:26 +0200
Subject: presentation/presentation.tex: Adding all relevant tables. Itemizing,
 where applicable. Adding more citations.

---
 presentation/presentation.tex | 480 +++++++++++++++++++++++++++++++++++++-----
 1 file changed, 426 insertions(+), 54 deletions(-)

(limited to 'presentation/presentation.tex')

diff --git a/presentation/presentation.tex b/presentation/presentation.tex
index 36fd3f7..9ce19fa 100644
--- a/presentation/presentation.tex
+++ b/presentation/presentation.tex
@@ -167,82 +167,146 @@ SuperCollider, Technische Universität Berlin, VBAP, WFS}
 \section{Spatial Audio Renderers}
   \begin{frame}
     \frametitle{What are they?}
-    Virtual auditory environment\\
-    Headphones and loudspeakers\\
-    Place sources inside and outside of listening area\\
+    \begin{itemize}
+      \item Virtual auditory environment\\
+      \item Headphones and loudspeakers\\
+      \item Place sources inside and outside of listening area\\
+    \end{itemize}
   \end{frame}
 
   \subsection{Algorithms}
     \begin{frame}
       \frametitle{What do they use?}
-      Dynamic Binaural Synthesis\\
-      Dynamic Binaural Room Synthesis\\
-      Vector Based Amplitude Panning\\
-      Ambisonics Amplitude Panning\\
-      Wave Field Synthesis\\
+      \begin{itemize}
+        \item (Dynamic) \gls{bs}\\
+        \item (Dynamic) \gls{brs}\\
+        \item \gls{vbap}\\
+        \item \gls{aap}\\
+        \item \gls{wfs}\\
+      \end{itemize}
     \end{frame}
 
   \subsection{Software Solutions}
     \begin{frame}
       \frametitle{What is available as free software?}
-      sWONDER\\
-      HoaLibrary\\
-      3Dj\\
-      WFSCollider\\
-      SoundScape Renderer\\
+      \begin{itemize}
+        \item sWONDER \citep{phdthesis:baalman2007}\\
+        \item HoaLibrary \citep{website:hoalibrary}\\
+        \item 3Dj \citep{mastersthesis:perezlopez2014}\\
+        \item WFSCollider \citep{manual:wfscollider}\\
+        \item \gls{ssr} \citep{website:ssr2016}\\
+      \end{itemize}
     \end{frame}
     \begin{frame}
       \frametitle{What are they used for?}
-      Scientific Research\\
-      Virtual Reality\\
-      Music\\
+      \begin{itemize}
+        \item Scientific Research\\
+        \item Virtual Reality\\
+        \item Music\\
+      \end{itemize}
     \end{frame}
 
 \section{Extending the SSR}
   \begin{frame}
     \frametitle{Why extend the SSR?}
-    Widespread use in scientific research\\
-    Large set of rendering algorithms\\
-    Still maintained\\
-    Possible candidate for large-scale WFS systems at TU Berlin\\
-    Extending user base\\
+    \begin{itemize}
+      \item Widespread use in scientific research\\
+      \item Large set of rendering algorithms\\
+      \item Still maintained\\
+      \item Possible candidate for medium/ large scale \gls{wfs} systems at
+        \gls{tu-berlin}\\
+      \item Extending user base\\
+    \end{itemize}
   \end{frame}
 
   \subsection{Use Cases}
     \begin{frame}
       \frametitle{Research}
-      BRS: \citet{mastersthesis:ackermannandilse2015},
-      \citet{mastersthesis:boehm2015} or \citet{mastersthesis:grigoriev2017}\\
-      WFS: \citet{bachelorsthesis:koslowski2013}\\
+      \begin{itemize}
+        \item \gls{brs}: \citet{mastersthesis:ackermannandilse2015},
+          \citet{mastersthesis:boehm2015} or
+          \citet{mastersthesis:grigoriev2017}\\
+        \item \gls{wfs}: \citet{bachelorsthesis:koslowski2013}\\
+      \end{itemize}
     \end{frame}
 
   \subsection{Current Capabilities}
     \begin{frame}
       \frametitle{Remote Controlling}
-      XML formatted string over TCP/IP socket\\
-      OSC through PureData\\
+      \begin{itemize}
+        \item XML formatted string over TCP/IP socket\\
+        \item \gls{osc} through \gls{pd} \citep{inproceedings:puckette1997}\\
+      \end{itemize}
     \end{frame}
     \begin{frame}
       \frametitle{Interaction}
-      GUI\\
-      No direct interaction between instances\\
-      Controlling multiple instances with PureData\\
+      \begin{itemize}
+        \item \gls{gui}\\
+        \item No direct interaction between instances\\
+        \item Controlling multiple instances with \gls{pd}\\
+      \end{itemize}
     \end{frame}
 
   \subsection{OSC Interface}
     \begin{frame}
       \frametitle{Why another interface?}
-      OSC natively\\
-      Inter-instance communication\\
-      Client-Server architecture\\
-      Controlling multiple instances with an SSR or other OSC capable
-      software\\
+      \begin{itemize}
+        \item \gls{osc} natively (using liblo \citep{website:liblo2017}): Clean
+          message interface\\
+        \item Inter-instance communication\\
+        \item Client-Server architecture\\
+        \item Controlling multiple instances with an \gls{ssr} or other
+          \gls{osc} capable software\\
+      \end{itemize}
     \end{frame}
     \begin{frame}
       \frametitle{Publisher/Subscriber}
       \includegraphics[scale=0.4, trim = 6mm 91mm 12mm 10mm, clip]
         {ssr-publisher-with-all-subscribers.pdf}
     \end{frame}
+    \begin{frame}[fragile]
+      \frametitle{\gls{osc}}
+      \begin{table}[!htb]
+        \renewcommand{\arraystretch}{1.2}
+        \scriptsize
+        \centering
+        \rowcolors{2}{table-background-one}{table-background-two}
+        \begin{tabular}{ p{2cm} | p{8cm} }
+          \textbf{\gls{osc} type tag} & \textbf{Type} \\
+          \hline
+          \texttt{i} & \mintinline{c++}{int32} \\
+          \texttt{f} & \mintinline{c++}{float32} \\
+          \texttt{s} & \gls{osc}-string \\
+          \texttt{b} & \gls{osc}-blob \\
+          \hline
+          \hline
+          \texttt{h} & 64 bit big-endian two's complement integer\\
+          \texttt{t} & \gls{osc}-timetag\\
+          \texttt{d} & 64 bit (“double”) IEEE 754 floating point number\\
+          \texttt{S} & Alternate type represented as an \gls{osc}-string (for
+          example, for systems that differentiate “symbols” from “strings”)\\
+          \texttt{c} & An \gls{ascii} character, sent as 32 bits\\
+          \texttt{r} & 32 bit RGBA color\\
+          \texttt{m} & 4 byte \gls{midi} message. Bytes from MSB to LSB are:
+          port id, status byte, data1, data2\\
+          \texttt{T} & True. No bytes are allocated in the argument data.\\
+          \texttt{F} & False. No bytes are allocated in the argument data.\\
+          \texttt{N} & Nil. No bytes are allocated in the argument data.\\
+          \texttt{I} & Infinitum. No bytes are allocated in the argument
+          data.\\
+          \texttt{[} & Indicates the beginning of an array. The tags
+            following are for data in the Array until a close brace tag is
+            reached.\\
+          \texttt{]} & Indicates the end of an array.\\
+        \end{tabular}
+        \caption{Acronyms (type tags) for atomic data types, used in
+        \gls{osc} messages and bundles \citep{website:oscv1.0}.}\\
+        The first four types define the standard \gls{osc} type tags, which
+        should be understood by all implementations. The remaining are
+        non-standard types, that are implemented by most (e.g.\ liblo
+        implements all but array and RGBA color type).
+      \end{table}
+    \end{frame}
 
   \subsection{Setups}
     \begin{frame}
@@ -290,7 +354,7 @@ SuperCollider, Technische Universität Berlin, VBAP, WFS}
 
   \subsection{Message Interface}
     \begin{frame}[fragile]
-      \frametitle{Message Interface}
+      \frametitle{Alive, Message Level, Subscribe (Server)}
       \begin{table}[!htb]
         \renewcommand{\arraystretch}{1.2}
         \scriptsize
@@ -326,31 +390,329 @@ SuperCollider, Technische Universität Berlin, VBAP, WFS}
       \end{table}
     \end{frame}
 
+    \begin{frame}
+      \frametitle{Message Level, Poll (Client)}
+      \begin{table}[!htb]
+        \renewcommand{\arraystretch}{1.2}
+        \scriptsize
+        \centering
+        \rowcolors{2}{table-background-one}{table-background-two}
+        \begin{tabular}{ p{2cm} | p{1cm} | p{3.5cm} | p{3cm} }
+          \textbf{Path} & \textbf{Types} & \textbf{Description} &
+          \textbf{Example}\\
+          \hline
+          \texttt{/message\_level} & i & Set message level of sender (the
+          server) & \texttt{[/message\_level, 1]} \\
+          \texttt{/poll} & & Poll client (continously sent), triggering
+          subscribe (see Table~\ref{tab:ssr-osc-subscribe}) &
+          \texttt{[/poll]} \\
+        \end{tabular}
+        \caption{\gls{osc} messages relevant for polling and setting of
+          message levels for servers subscribed to.\\
+        }
+        \label{tab:ssr-osc-client-poll-message-level}
+      \end{table}
+    \end{frame}
+    \begin{frame}[fragile]
+      \frametitle{Processing, Tracker, Transport}
+      \begin{table}[!htb]
+        \renewcommand{\arraystretch}{1.2}
+        \scriptsize
+        \rowcolors{2}{table-background-one}{table-background-two}
+        \begin{tabular}{ p{2.1cm} | p{0.8cm} | p{3.5cm} | p{2.5cm} }
+          \textbf{Path} & \textbf{Types} & \textbf{Description} &
+          \textbf{Example}\\
+          \hline
+          \texttt{/processing/state} & F & Unset processing state &
+          \texttt{[/processing/state, false]} \\
+          \texttt{/processing/state} & T & Set processing state &
+          \texttt{[/processing/state, true]} \\
+          \texttt{/tracker/reset} & & Reset tracker &
+          \texttt{[/tracker/reset]} \\
+          \texttt{/transport/rewind} & & Rewind the \gls{jack} transport &
+          \texttt{[/transport/rewind]} \\
+          \texttt{/transport/seek} & s & Seek to time code in
+          \gls{jack} transport & \texttt{[/transport/seek, “42:00:00”]} \\
+          \texttt{/transport/state} & F & Unset \gls{jack} transport
+          state & \texttt{[/transport/state, false]} \\
+          \texttt{/transport/state} & T & Set \gls{jack} transport
+          state & \texttt{[/transport/state, true]} \\
+        \end{tabular}
+        \caption{\gls{osc} messages relevant for processing, tracker and
+          (\gls{jack}) transport related settings.\\
+        }
+        \label{tab:ssr-osc-processing-tracker-transport}
+      \end{table}
+    \end{frame}
+    \begin{frame}
+      \frametitle{Reference}
+      \begin{table}[!htb]
+        \renewcommand{\arraystretch}{1.2}
+        \scriptsize
+        \centering
+        \rowcolors{2}{table-background-one}{table-background-two}
+        \begin{tabular}{ p{3.2cm} | p{0.6cm} | p{2.5cm} | p{3.3cm} }
+          \textbf{Path} & \textbf{Types} & \textbf{Description} &
+          \textbf{Example}\\
+          \hline
+          \texttt{/reference/orientation} & f & Set azimuth of reference
+          point & \texttt{[/reference/orientation, -90.0]} \\
+          \texttt{/reference/position} & ff & Set position of reference &
+          \texttt{[/reference/position, 1.5, 2.0]} \\
+          \texttt{/reference\_offset/orientation} & f & Set azimuth of
+          reference offset position &
+          \texttt{[/reference\_offset/orientation, -90.0]} \\
+          \texttt{/reference\_offset/position} & ff & Set position of
+          reference offset & \texttt{[/reference\_offset/position, 1.5,
+          2.0]}\\
+        \end{tabular}
+        \caption{\gls{osc} messages relevant for reference management.\\
+        }
+        \label{tab:ssr-osc-reference}
+      \end{table}
+    \end{frame}
+    \begin{frame}
+      \frametitle{Scene}
+      \begin{table}[!htb]
+        \renewcommand{\arraystretch}{1.2}
+        \scriptsize
+        \centering
+        \rowcolors{2}{table-background-one}{table-background-two}
+        \begin{tabular}{ p{3.3cm} | p{0.7cm} | p{2.5cm} | p{3.3cm} }
+          \textbf{Path} & \textbf{Types} & \textbf{Description} &
+          \textbf{Example} \\
+          \hline
+          \texttt{/scene/amplitude\_reference
+          \_distance} & f & Set amplitude
+          reference distance. &
+          \texttt{[/scene/amplitude\_reference
+          \_distance, 6.0]}\\
+          \texttt{/scene/auto\_rotate\_sources} & F & Disable automatic
+          rotation of sources. & \texttt{[/scene/auto\_rotate\_sources,
+          false]}\\
+          \texttt{/scene/auto\_rotate\_sources} & T & Enable automatic
+          rotation of sources. & \texttt{[/scene/auto\_rotate\_sources,
+          true]}\\
+          \texttt{/scene/clear} & & Delete all sources &
+          \texttt{[/scene/clear]}\\
+          \texttt{/scene/decay\_exponent} & f & Set amplitude decay exponent
+          in virtual space ($1/r^{exp}$). & \texttt{[/scene/decay\_exponent,
+          2.0]}\\
+          \texttt{/scene/load} & s & Load scene from \gls{asdf} file. &
+          \texttt{[/scene/load, “example.asd”]}\\
+          \texttt{/scene/master\_signal\_level} & f & Set the renderers
+          signal level. & \texttt{[/scene/master\_signal\_level, -20]}\\
+          \texttt{/scene/save} & s & Save scene to \gls{asdf} file. &
+          \texttt{[/scene/save, “example.asd”]}\\
+          \texttt{/scene/volume} & f & Set scene master volume. &
+          \texttt{[/scene/volume, 0.23]}\\
+        \end{tabular}
+        \caption{\gls{osc} messages relevant for scene management.\\
+        }
+        \label{tab:ssr-osc-scene}
+      \end{table}
+    \end{frame}
+    \begin{frame}
+      \frametitle{Source I}
+      \begin{table}[!htb]
+        \renewcommand{\arraystretch}{1.2}
+        \scriptsize
+        \centering
+        \rowcolors{2}{table-background-one}{table-background-two}
+        \begin{tabular}{ p{2.4cm} | p{1.0cm} | p{2.5cm} | p{3.3cm} }
+          \textbf{Path} & \textbf{Types} & \textbf{Description} &
+          \textbf{Example} \\
+          \hline
+          \texttt{/source/delete} & i & Delete source with given id &
+          \texttt{[/source/delete, 1]}\\
+          \texttt{/source/file\_channel} & ii & Set a source's file channel &
+          \texttt{[/source/file\_channel, 1, 2]}\\
+          \texttt{/source/file\_name\_ or\_port\_number} & is & Set a source's
+          file name or port number &
+          \texttt{[/source/file\_name\_ or\_port\_number, 1, “1”]}\\
+          \texttt{/source/port\_name } & is & Set a source's \gls{jack} input
+          port name & \texttt{[/source/port\_name, 1, “system:capture\_2”]}\\
+          \texttt{/source/gain} & if & Set a source's gain on a linear scale
+          (0.0 - inf) & \texttt{[/source/gain, 1, 0.2]}\\
+          \texttt{/source/model} & is & Set a source's model &
+          \texttt{[/source/model, 1, “point”]}\\
+          \texttt{/source/mute} & iF & Unmute a source &
+          \texttt{[/source/mute, 1, false]}\\
+          \texttt{/source/mute} & iT & Mute a source &
+          \texttt{[/source/mute, 1, true]}\\
+          \texttt{/source/name} & is & Set a source's name &
+          \texttt{[/source/name, 1, “Daisy”]}\\
+          \texttt{/source/new} & i & Create a new source stub using id &
+          \texttt{[/source/new, 1]}\\
+          \texttt{/source/new} & sssffffTFF & Create a new source
+          (auto-generated id) with name, model, port number, X-coordinate,
+          Y-coordinate, orientation, gain, movability, orientation movability
+          and mute status & \texttt{[/source/new, “Daisy”, “point”, “1”, 1.0,
+          2.5, 90.0, 0.2, true, false, false]} \\
+        \end{tabular}
+        \caption{\gls{osc} messages relevant for source management.\\
+        }
+        \label{tab:ssr-osc-source-1}
+      \end{table}
+    \end{frame}
+    \begin{frame}
+      \frametitle{Source II}
+      \begin{table}[!htb]
+        \renewcommand{\arraystretch}{1.2}
+        \scriptsize
+        \centering
+        \rowcolors{2}{table-background-one}{table-background-two}
+        \begin{tabular}{ p{2.4cm} | p{1.0cm} | p{2.5cm} | p{3.3cm} }
+          \textbf{Path} & \textbf{Types} & \textbf{Description} &
+          \textbf{Example} \\
+          \hline
+          \texttt{/source/new} & sssffffisTFF & Create a new source
+          (auto-generated id) with name, model, port number, X-coordinate,
+          Y-coordinate, orientation, gain, file channel, properties file,
+          movability, orientation movability and mute status &
+          \texttt{[/source/new, “Daisy”, “point”, “1”, 1.0, 2.5, 90.0, 0.2,
+          2, “properties.xml”, true, false, false]} \\
+          \texttt{/source/orientation} & if & Set a source's orientation &
+          \texttt{[/source/orientation, 1, -90.0]}\\
+          \texttt{/source/position} & iff & Set a source's position &
+          \texttt{[/source/position, 1, 1.5, 2.0]}\\
+          \texttt{/source/position\_fixed} & iF & Set a source movable &
+          \texttt{[/source/position\_fixed, 1, false]}\\
+          \texttt{/source/position\_fixed} & iT & Set a source immovable &
+          \texttt{[/source/position\_fixed, 1, true]}\\
+          \texttt{/source/properties\_file} & is & Set a source's properties
+          file & \texttt{[/source/properties\_file, 1,
+          “source-properties.xml”]}\\
+        \end{tabular}
+        \caption{\gls{osc} messages relevant for source management.\\
+        }
+        \label{tab:ssr-osc-source-2}
+      \end{table}
+    \end{frame}
+    \begin{frame}
+      \frametitle{Update (Server) I}
+      \begin{table}[!htb]
+        \renewcommand{\arraystretch}{1.2}
+        \scriptsize
+        \centering
+        \rowcolors{2}{table-background-one}{table-background-two}
+        \begin{tabular}{ p{4.6cm} | p{0.7cm} | p{4.0cm} }
+          \textbf{Path} & \textbf{Types} & \textbf{Description} \\
+          \hline
+          \texttt{/update/cpu\_load} & f & \gls{cpu} load changes.\\
+          \texttt{/update/processing/state} & T & Processing state is set.\\
+          \texttt{/update/processing/state} & F & Processing state is
+          unset.\\
+          \texttt{/update/reference/orientation} & f & Reference orientation
+          changes.\\
+          \texttt{/update/reference/position} & ff & Reference position
+          changes.\\
+          \texttt{/update/reference\_offset/orientation} & f & Reference
+          offset orientation changes.\\
+          \texttt{/update/reference\_offset/position} & ff & Reference offset
+          position changes.\\
+          \texttt{/update/scene/amplitude\_reference\_distance} & f &
+          Amplitude reference distance changes.\\
+          \texttt{/update/scene/auto\_rotate\_sources} & T & Auto rotation of
+          sources is set.\\
+          \texttt{/update/scene/auto\_rotate\_sources} & F & Auto rotation of
+          sources is unset.\\
+          \texttt{/update/scene/decay\_exponent} & f & The scene's decay
+          exponent has changed.\\
+          \texttt{/update/scene/master\_signal\_level} & f & Master signal
+          level has changed.\\
+          \texttt{/update/scene/sample\_rate} & i & Sample rate of the scene
+          changed.\\
+          \texttt{/update/scene/volume} & f & Volume of the scene has
+          changed.\\
+          \texttt{/update/source/delete} & i & A source with given id was
+          deleted. \\
+          \texttt{/update/source/file\_channel} & ii & A source's file
+          channel was set.\\
+          \texttt{/update/source/file\_name\_or\_port\_number} & is & A
+          source's file name or port number was set.\\
+          \texttt{/update/source/gain} & if & A source's gain was set.\\
+        \end{tabular}
+        \caption{\gls{osc} messages for updating information on \gls{cpu} load,
+          processing, reference, scene, source, and transport of clients on a
+          server.\\
+        }
+        \label{tab:ssr-osc-update-1}
+      \end{table}
+    \end{frame}
+    \begin{frame}
+      \frametitle{Update (Server) II}
+      \begin{table}[!htb]
+        \renewcommand{\arraystretch}{1.2}
+        \scriptsize
+        \centering
+        \rowcolors{2}{table-background-one}{table-background-two}
+        \begin{tabular}{ p{3.3cm} | p{0.7cm} | p{3.3cm} }
+          \textbf{Path} & \textbf{Types} & \textbf{Description} \\
+          \hline
+          \texttt{/update/source/length} & ii & A source's length was set.\\
+          \texttt{/update/source/level} & if & A source's output level has
+          changed.\\
+          \texttt{/update/source/model} & is & A source's model was set.\\
+          \texttt{/update/source/mute} & iF & A source was unmuted.\\
+          \texttt{/update/source/mute} & iT & A source was muted.\\
+          \texttt{/update/source/name} & is & A source's name was set.\\
+          \texttt{/update/source/orientation} & if & A source's orientation
+          was set. \\
+          \texttt{/update/source/new} & i & A new source with given id was
+          created. \\
+          \texttt{/update/source/port\_name} & is & A source's \gls{jack}
+          port\_name was set. \\
+          \texttt{/update/source/position} & iff & A source's position was
+          set. \\
+          \texttt{/update/source/position\_fixed} & iF & A source was set to
+          be movable. \\
+          \texttt{/update/source/position\_fixed} & iT & A source was set to
+          be immovable. \\
+          \texttt{/update/source/properties\_file} & is & A source's
+          properties\_file was set.\\
+          \texttt{/update/transport/seek} & s & \gls{jack} transport seeked
+          to a timecode position.\\
+          \texttt{/update/transport/state} & F & \gls{jack} transport was
+          stopped.\\
+          \texttt{/update/transport/state} & T & \gls{jack} transport was
+          started.\\
+        \end{tabular}
+        \caption{\gls{osc} messages for updating information on \gls{cpu} load,
+          processing, reference, scene, source, and transport of clients on a
+          server.\\
+        }
+        \label{tab:ssr-osc-update-2}
+      \end{table}
+    \end{frame}
+
 \section{Demo}
-  \begin{frame}[fragile,allowframebreaks]
+  \begin{frame}[fragile]
     \frametitle{Sensors2OSC\footnote{\href{https://sensors2.org/osc/}{https://sensors2.org/osc/}}}
-    Sending \gls{osc} messages from mobile phone to \gls{supercollider}\\
-    Evaluating and forwarding data to an \gls{ssr} server instance\\
-    \\
-    \vspace{0.23cm}
-    Starting an \gls{ssr} client
-    \begin{mdframed}
-      \begin{minted}[fontsize=\footnotesize]{shell}
+    \begin{itemize}
+      \item{Starting an \gls{ssr} client
+        \begin{mdframed}
+          \begin{minted}[fontsize=\footnotesize]{shell}
 ssr-binaural -p “50002”
-      \end{minted}
-    \end{mdframed}
-    \vspace{0.23cm}
-    Starting an \gls{ssr} server
-    \begin{mdframed}
-      \begin{minted}[fontsize=\footnotesize]{shell}
+          \end{minted}
+        \end{mdframed}}
+      \item{Starting an \gls{ssr} server (with initial client)
+        \begin{mdframed}
+          \begin{minted}[fontsize=\footnotesize]{shell}
 ssr-aap -N “server” -C “127.0.0.1:50002”
-      \end{minted}
-    \end{mdframed}
+          \end{minted}
+        \end{mdframed}
+      }
+      \item Sending \gls{osc} messages from mobile phone to \gls{supercollider}\\
+      \item Evaluating and forwarding data to the \gls{ssr} server instance\\
+    \end{itemize}
   \end{frame}
 
 \section{Future Work}
   \begin{frame}
     \frametitle{Future Work}
+    Code Adoption!!!\\
+    User Manual Extension\\
     Non-Renderer\\
     Alien-Loudspeaker\\
     Status Messages\\
@@ -361,7 +723,17 @@ ssr-aap -N “server” -C “127.0.0.1:50002”
     Network Enabled Head Tracking\\
   \end{frame}
 
-\scriptsize
-\bibliographystyle{../help/FG_AK_English_AuthorYear.bst}
-\bibliography{../bib/ssr-networking}
+  \begin{frame}
+    \frametitle{References}
+    \scriptsize
+    \bibliographystyle{../help/FG_AK_English_AuthorYear.bst}
+    \bibliography{../bib/ssr-networking}
+  \end{frame}
+
+  \begin{frame}
+    \frametitle{Glossary/ Acronyms}
+    \scriptsize
+    \printglossaries
+  \end{frame}
+
 \end{document}
-- 
cgit v1.2.3-54-g00ecf

